Industrial LC™Standard [IND LC STANDARD PU]

|  |  |
| --- | --- |
| Backrest   * 15" wide by 13" high * Dual Curve Polyurethane Backrest   Arms   * [Click here](http://ergocentric.com/resource/arms) to view options   Seat   * High Resilient Polyurethane Foam * Seat Pan 18.5" wide by 17" deep   **Options:**   * Raised pattern design for both seat and backrest reduces slippage for additional safety. Backrest has a handle for easy maneuvering of the chair [RP]   Standard Mechanism   * Back Angle Adjustment * Back Height Adjustment * Back Pivot   Pneumatic Lift (Seat Height)   * 200 mm Knurled Pneumatic Lift, Dual Height Adjustment System (seat height 7.5" of adjustment between 2"- 35.25") | Base/Glides/Casters   * 26" Multi-level Spider Base with Durable Urethane Coating * ½" Industrial Glides * Footrests 3", 6.5", 9", 12" high   **Options:**   * 22" Chrome 22 Base has an 18" oval tube footring built in for durability [C22] * 30" Diameter Flat Bi-level Footrest (30"W x 20.5"H) [30FBLFR] * Nylon Casters (adds 1.5" to seat height) [NC] * Urethane Casters (adds 1.5" to seat height) [UC] * Single Wheel Casters (adds 1.5" to seat height) [SW] * Single Wheel Urethane Casters  (adds 1.5" to seat height) [SWU] * Lock-on Urethane Casters  (adds 1.5" to seat height) [LON] * Lock-off urethane casters  (adds 1.5" to seat height)  [LOF] * 1/2" Flat Glides [HG] * 2 1/4" Glides  (adds 1.5" to seat height)  [2G] |

