airCentric™Boardroom [air-BR]

|  |  |
| --- | --- |
| Backrest   * 5" Patented Back Height Adjustment System * Front Upholstered Dual Curve Backrest (19"w x 24"h) * Plastic Back Cap with Airflow Vents * Proprietary Airflow Molded Polyurethane Foam and Structure   Arms   * [Click here](http://ergocentric.com/resource/arms) to view options   Seat   * Tailored Upholstery on Seat Pan (20”w x 19”d) * Proprietary Airflow Molded Polyurethane Foam and Structure   **Options:**   * Extra Long Non-Airflow Seat (20”w x 21”d) [XLS] * Small Non-Airflow Seat (18.5”w x 17”d) [SS] * Triple Density Foam (adds ¼” to seat width and depth) (Not available on airCentric seat options) [TDF] * Standard Non-Airflow Seat (20”w x 19”d) [LS] * airCentric Plus Size Seat (22”w x 19”d) [ACPS]] * airCentric Small Seat (18.5”w x 17”d) [ACSS]   Boardroom Mechanism   * Adjustable Spring Tension * Seat Height * Single Tilt Lock Free Float   Pneumatic Lift (Seat Height)   * 125 mm Pneumatic Lift (16" - 21")   **Options:**   * 80 mm Pneumatic Lift (only available with 26” Glass Reinforced Nylon Base) (15”-18”) [80mm] * 100 mm Pneumatic Lift (15.5”-19”) [100mm] * 140 mm Pneumatic Lift (17”-22.5”) [140mm] * Memory Gas Column (17”) [MGC] | Base/Glides/Casters   * 25" Glass Reinforced Nylon High Profile Base * 5 Dual Wheel Nylon Carpet Casters   **Options:**   * Chrome Accent Casters [CAC] * 26” Polished Aluminum Base [PB] * Urethane Casters [UC] * 26” Glass Reinforced Nylon Base [26NB] |