tCentric Hybrid™Boardroom [t-BR]

|  |  |
| --- | --- |
| Backrest   * 5" Patented Back Height Adjustment System Dual Curve Mesh Backrest (19"w x 25"h)   Arms   * [Click here](http://ergocentric.com/resource/arms) to view options   Seat   * Seat Pan 20" wide by 19" deep * Dual Density Molded Polyurethane   Boardroom Mechanism   * Adjustable Spring Tension * Seat Height * Single Tilt Lock Free Float   Pneumatic Lift (Seat Height)   * 125 mm Pneumatic Lift (16" - 21")   **Options:**   * 100 mm Pneumatic Lift (15”-18.5”) [100mm] * 100 mm Pneumatic Lift Chrome (14.75”-17.75”) [100mmCH] * 125 mm Pneumatic Lift Chrome (15”-18.5”) [125mmCH] * 140 mm Pneumatic Lift Chrome (16.5”-22) [140mmCH] * 80 mm Pneumatic Lift (14.75”-17.75”) [80mm] | Base/Glides/Casters   * 26" Glass Reinforced Nylon High Profile Base 2 * 5 Dual Wheel Nylon Carpet Casters 2   **Options:**   * Chrome Accent Casters [CAC] * 26" Polished Aluminum High Profile Base [PB2] * Urethane Caster [UC2]   Additional Options   * Adjustable Headrest [AHR] * CooltoTouch Lumbar Support (12"w x 6"h) [TLS] * CooltoTouch Lumbar Support with Air Lumbar [TLSAL]   Measurements / Overall Dimensions  Boxed Weight/Size (56 lbs./11.7 cu.ft) |