tCentric Hybrid™Synchro Glide [t-SG]

|  |  |
| --- | --- |
| Backrest   * 5" Patented Back Height Adjustment System Dual Curve Mesh Backrest (19"w x 25"h)   Arms   * [Click here](http://ergocentric.com/resource/arms) to view options   Seat   * Eight Ply Hardwood Seat Structure * Seat Pan 20" wide by 19" deep * Dual Density Molded Polyurethane   **Options:**   * Memory Foam Seat [EA] * Extra Long Seat (20"w x 21"d) [XLS] * Small Seat (18.5"wx17"d) [SS] * Triple Density Foam Seat (Adds 1/4" to seat width and depth) [TDF]   Synchro Glide Mechanism   * 2.5” Depth Adjustable Seat Slider * Adjustable Spring Tension * Free Float * Independent Back Angle Adjustment * Seat Tilt Lock Out * Synchro 2:1 Ratio   Pneumatic Lift (Seat Height)   * 125 mm Pneumatic Lift (18" - 23")   **Options:**   * 100 mm Pneumatic Lift (17.5" - 21") *100mm* * 140 mm Pneumatic Lift (19" – 24.5") *140mm* * 80 mm Pneumatic Lift (17.25" - 20.25") *80mm* * 100 mm Pneumatic Lift Chrome (17.5" - 21") *100mmCH* * 125 mm Pneumatic Lift Chrome (18” -23”) *25mmCH* * 140 mm Pneumatic Lift Chrome (19"-24.5") *140mmCH* | Base/Glides/Casters   * 26" Glass Reinforced Nylon High Profile Base 2 * 5 Dual Wheel Nylon Carpet Casters 2   **Options:**   * Chrome Accent Casters [CAC] * 26" Polished Aluminum High Profile Base [PB2] * Urethane Caster [UC2]   Additional Options   * Adjustable Headrest [AHR] * CooltoTouch Lumbar Support (12"w x 6"h) [TLS] * CooltoTouch Lumbar Support with Air Lumbar [TLSAL]   Measurements / Overall Dimensions  Boxed Weight/Size (56 lbs./11.7 cu.ft) |