tCentric Hybrid™Synchro Glide [t-SG]

|  |  |
| --- | --- |
| Backrest* 5" Patented Back Height Adjustment SystemDual Curve Mesh Backrest (19"w x 25"h)

Arms* [Click here](http://ergocentric.com/resource/arms) to view options

Seat* Eight Ply Hardwood Seat Structure
* Seat Pan 20" wide by 19" deep
* Dual Density Molded Polyurethane

**Options:*** Memory Foam Seat [EA]
* Extra Long Seat (20"w x 21"d) [XLS]
* Small Seat (18.5"wx17"d) [SS]
* Triple Density Foam Seat (Adds 1/4"to seat width and depth) [TDF]

Synchro Glide Mechanism* 2.5” Depth Adjustable Seat Slider
* Adjustable Spring Tension
* Free Float
* Independent Back Angle Adjustment
* Seat Tilt Lock Out
* Synchro 2:1 Ratio

Pneumatic Lift (Seat Height)* 125 mm Pneumatic Lift (18" - 23")

**Options:*** 100 mm Pneumatic Lift (17.5" - 21") *100mm*
* 140 mm Pneumatic Lift (19" – 24.5") *140mm*
* 80 mm Pneumatic Lift (17.25" - 20.25") *80mm*
* 100 mm Pneumatic Lift Chrome (17.5" - 21") *100mmCH*
* 125 mm Pneumatic Lift Chrome (18” -23”) *25mmCH*
* 140 mm Pneumatic Lift Chrome (19"-24.5") *140mmCH*
 | Base/Glides/Casters* 26" Glass Reinforced Nylon High Profile Base 2
* 5 Dual Wheel Nylon Carpet Casters 2

**Options:*** Chrome Accent Casters [CAC]
* 26" Polished Aluminum High Profile Base [PB2]
* Urethane Caster [UC2]

Additional Options* Adjustable Headrest [AHR]
* CooltoTouch Lumbar Support (12"w x 6"h) [TLS]
* CooltoTouch Lumbar Support with Air Lumbar [TLSAL]

Measurements / Overall DimensionsBoxed Weight/Size (56 lbs./11.7 cu.ft) |