geoCentric Stacker Armless [geo-STACKER]

|  |  |
| --- | --- |
| Backrest   * Backrest 18.25" wide by 12.5" high * Concealed Back Brackets (except when upholstered in vinyl or leather) * Dual Curve Backrest   Seat   * 17" Seat Height * Dual Curve Waterfall Seat * Seat Pan 18.5" wide by 19.5" deep | Base/Glides/Casters  **Options:**   * Nylon Stacker Casters [NSC] * Urethane Stacker Casters [USC] * Metal Sled base option with glass reinforced nylon glides (chair does not stack with sled base option) [SLED]   Frame   * 14 Gauge, 7/8" Steel Tube Frame * Black Textured Semi-Gloss Powder Coat Paint * Kick Back Legs for Stability with Durable Custom Glides   **Options**   * Chrome frame (CF) * Wall saver frame (SWS)   Additional Options   * Cal. 133 [Cal133] * Cart (23" wide by 29.75" long by 14.75" high) Stackable 6 units high without cart and 10 units high with cart [CART] * Ganging clips (set of 2) chair with arms [GC]   Measurements / Overall Dimensions  Boxed Weight/Size (21 lbs./13 cu.ft) |