ecoCentric™ MeshDedicated Task [eco-MESH-DT]

|  |  |
| --- | --- |
| Backrest* Mesh backrest (19.25”w x 23”h)
* 4” of adjustable lumbar support

Arms* [Click here](http://ergocentric.com/resource/arms) to view options

Seat* Eight Ply Hardwood Seat Structure
* High Resilient Polyurethane Foam
* Tailored Upholstery on seat Pan (20”w x 19”d)

**Options:*** 1.5” Seat Slider used with an Extra Small Seat [XSS]
* Memory Foam Seat [EA]
* Extra Small Seat (17.5”w x 15.5”d) (Recommended with TATA arm option) [XSS]
* Extra Long Seat (20”w x 21”d) [XLS]
* 2.5” Seat Slider (adds 1 ½” to seat height) [SSLF]
* Large Airflow Seat (20”w x 19”d) [LSAF]
* Small Airflow Seat (18.5”w x 17”d) [SSAF
* Small Seat (18.5”w x 17”d) [SS]
* Triple Density Foam Seat (Adds ¼” to seat width and depth) [TDF]

Dedicated Task Mechanism* Independent Back Angle Adjustment
* Seat Angle Adjustment
* Seat Height

Pneumatic Lift (Seat Height)* 125 mm Pneumatic Lift (15.5" – 20.5")

**Options:*** 80 mm Pneumatic Lift (only available with 26” glass reinforced nylon base)(14.75”-17.75”) [80mm]
* 100 mm Pneumatic Lift (15”-18.5”) [100mm]
* 140 mm Pneumatic Lift (16.5”-22”) [140mm]
 | Base/Glides/Casters* 25” Glass Reinforced Nylon High Profile Base
* 5 Dual Wheel Nylon Carpet Casters

**Options:*** 2 ¼” Glides [2G]
* 26” Glass Reinforced Nylon Base [26NB]
* Chrome Accent Casters [CAC]
* 26” Polished Aluminum Base [PB]
* Single Wheel Casters [SW]
* Single Wheel Urethane Casters [SWU]
* Urethane Casters [UC]

Additional Options* Tilt Mechanism (adds 2.5” of back height adjustment) [TILT]
* Adjustable Headrest [AHR]
* Cal. 133 [Cal133]

  |