ecoCentric™ MeshDedicated Task [eco-MESH-DT]

|  |  |
| --- | --- |
| Backrest   * Mesh backrest (19.25”w x 23”h) * 4” of adjustable lumbar support   Arms   * [Click here](http://ergocentric.com/resource/arms) to view options   Seat   * Eight Ply Hardwood Seat Structure * High Resilient Polyurethane Foam * Tailored Upholstery on seat Pan (20”w x 19”d)   **Options:**   * 1.5” Seat Slider used with an Extra Small Seat [XSS] * Memory Foam Seat [EA] * Extra Small Seat (17.5”w x 15.5”d) (Recommended with TATA arm option) [XSS] * Extra Long Seat (20”w x 21”d) [XLS] * 2.5” Seat Slider (adds 1 ½” to seat height) [SSLF] * Large Airflow Seat (20”w x 19”d) [LSAF] * Small Airflow Seat (18.5”w x 17”d) [SSAF * Small Seat (18.5”w x 17”d) [SS] * Triple Density Foam Seat (Adds ¼” to seat width and depth) [TDF]   Dedicated Task Mechanism   * Independent Back Angle Adjustment * Seat Angle Adjustment * Seat Height   Pneumatic Lift (Seat Height)   * 125 mm Pneumatic Lift (15.5" – 20.5")   **Options:**   * 80 mm Pneumatic Lift (only available with 26” glass reinforced nylon base)(14.75”-17.75”) [80mm] * 100 mm Pneumatic Lift (15”-18.5”) [100mm] * 140 mm Pneumatic Lift (16.5”-22”) [140mm] | Base/Glides/Casters   * 25” Glass Reinforced Nylon High Profile Base * 5 Dual Wheel Nylon Carpet Casters   **Options:**   * 2 ¼” Glides [2G] * 26” Glass Reinforced Nylon Base [26NB] * Chrome Accent Casters [CAC] * 26” Polished Aluminum Base [PB] * Single Wheel Casters [SW] * Single Wheel Urethane Casters [SWU] * Urethane Casters [UC]   Additional Options   * Tilt Mechanism (adds 2.5” of back height adjustment) [TILT] * Adjustable Headrest [AHR] * Cal. 133 [Cal133] |