ecoCentric™ MeshMulti Tilt [eco-MESH-MT2]

|  |  |
| --- | --- |
| Backrest   * Mesh backrest (19.25”w x 23”h) * 4” of adjustable lumbar support   Arms   * [Click here](http://ergocentric.com/resource/arms) to view options   Seat   * Eight Ply Hardwood Seat Structure * High Resilient Polyurethane Foam * Tailored Upholstery on Seat Pan 20”w x 19”d   **Options:**   * Memory Foam Seat [EA] * Extra Long Seat (20”w x 21”d) [XLS] * Large Airflow Seat (20”w x 19”d) [LSAF] * Small Airflow Seat (18.5”w x 17”d) [SSAF] * Small Seat (18.5”w x 17”d) [SS] * Triple Density Foam Seat (Adds ¼” to seat width and depth) [TDF]   Multi Tilt Mechanism   * 2.5” Depth Adjustable Seat Slider * Adjustable Spring Tension * Back Angle Adjustment * Infinite Forward Tilt Lock Out * Infinite Lock Free Float   Pneumatic Lift (Seat Height)   * 125 mm Pneumatic Lift (16.5" – 21.5")   **Options:**   * 80 mm Pneumatic Lift (only available with 26” base [26NB] (15.75”-18.75”) [80mm] * 100 mm Pneumatic Lift (16”-19.5”) [100mm] * 140 mm Pneumatic Lift (17.5”-23”) [140mm] | Base/Glides/Casters   * 25” Glass Reinforced Nylon High Profile Base * 5 Dual Wheel Nylon Carpet Casters   **Options:**   * 26” Glass Reinforced Nylon Base [26NB] * Chrome Accent Casters [CAC] * 26” Polished Aluminum Base [PB] * Single Wheel Casters [SW] * Single Wheel Urethane Casters [SWU] * Urethane Casters [UC] * 2 ¼” Glides [2G]   Additional Options   * 24 Hour Multi Tilt Mechanism (Warranted for 24 hour use up to a weight of 280 lbs.) [24MT] * Adjustable Headrest [AHR] * Cal. 133 [Cal133] |