Industrial LC™Standard [IND LC STANDARD PU]

|  |  |
| --- | --- |
| Backrest* 15" wide by 13" high
* Dual Curve Polyurethane Backrest

Arms* [Click here](http://ergocentric.com/resource/arms) to view options

Seat* High Resilient Polyurethane Foam
* Seat Pan 18.5" wide by 17" deep

**Options:*** Raised pattern design for both seat and backrest reduces slippage for additional safety. Backrest has a handle for easy maneuvering of the chair [RP]

Standard Mechanism* Back Angle Adjustment
* Back Height Adjustment
* Back Pivot

Pneumatic Lift (Seat Height)* 200 mm Knurled Pneumatic Lift, Dual Height Adjustment System (seat height 7.5" of adjustment between 2"- 35.25")

 | Base/Glides/Casters* 26" Multi-level Spider Base with Durable Urethane Coating
* ½" Industrial Glides
* Footrests 3", 6.5", 9", 12" high

**Options:*** 22" Chrome 22 Base has an 18" oval tube footring built in for durability [C22]
* 30" Diameter Flat Bi-level Footrest (30"W x 20.5"H) [30FBLFR]
* Nylon Casters (adds 1.5" to seat height) [NC]
* Urethane Casters (adds 1.5" to seat height) [UC]
* Single Wheel Casters (adds 1.5" to seat height) [SW]
* Single Wheel Urethane Casters (adds 1.5" to seat height) [SWU]
* Lock-on Urethane Casters (adds 1.5" to seat height) [LON]
* Lock-off urethane casters (adds 1.5" to seat height) [LOF]
* 1/2" Flat Glides [HG]
* 2 1/4" Glides (adds 1.5" to seat height) [2G]
* Height Adjustable Footring [ERGOFR]
 |