Spider Sit Stand[SPIDER SIT STAND]

|  |  |
| --- | --- |
| Seat* Adjustable Spring Tension
* Infinite Lock Tilting Seat Pan
* Upholstered sit stand seat (17.5" w x 15.5" d)

**Options:*** ergoCentric+Guard Sealed Seat (includes under seat pan) [EGUSS]

Pneumatic Lift (Seat Height)* 200 mm Knurled Pneumatic Lift, Dual Height Adjustment System (seat height 7.5" of adjustment between 21"-33.5")

 | Base/Glides/Casters* 1/2" Industrial Glides
* 22 Bi-Level Spider Base has highly durable anti-scuff textured powder coating and embossed steel treads on footrests
* Footrest 7", 9.5" high

**Options:*** 22" Chrome 22 Base has an 18" oval tube footring built in for durability [C22]
* Lock-on Urethane Casters (adds 1.5" to seat height) [LON]
* 2 1/4" Glides (adds 1.5" to seat height) [2G]

Additional Options* 6" ergoCentric+Guard No Slip Strip on front of seat [ANTSPU]
* Cal. 133 [Cal133]
* Anti Static (Available in fabric and vinyl only) [ANTISTATIC]
* Height Adjustable Footring [ERGOFR]
 |