Spider Sit Stand[SPIDER SIT STAND]

|  |  |
| --- | --- |
| Seat   * Adjustable Spring Tension * Infinite Lock Tilting Seat Pan * Upholstered sit stand seat (17.5" w x 15.5" d)   **Options:**   * ergoCentric+Guard Sealed Seat (includes under seat pan) [EGUSS]   Pneumatic Lift (Seat Height)   * 200 mm Knurled Pneumatic Lift, Dual Height Adjustment System (seat height 7.5" of adjustment between 21"-33.5") | Base/Glides/Casters   * 1/2" Industrial Glides * 22 Bi-Level Spider Base has highly durable anti-scuff textured powder coating and embossed steel treads on footrests * Footrest 7", 9.5" high   **Options:**   * 22" Chrome 22 Base has an 18" oval tube footring built in for durability [C22] * Lock-on Urethane Casters (adds 1.5" to seat height) [LON] * 2 1/4" Glides (adds 1.5" to seat height) [2G]   Additional Options   * 6" ergoCentric+Guard No Slip Strip on front of seat [ANTSPU] * Cal. 133 [Cal133] * Anti Static (Available in fabric and vinyl only) [ANTISTATIC] * Height Adjustable Footring [ERGOFR] |