airCentric™2

|  |  |
| --- | --- |
| Counter Height\* | Midnight Black [air2-CH/air2S-CH] |
| Light Grey [air2-CHG/air2S-CHG] |
|  | |
| Backrest:  Midnight Black / Light Grey   * 5" Patented Back Height Adjustment System * Plastic Back Cap with Airflow Vents [air2] * Solid Back Cap [air2S] * Proprietary Airflow Molded Polyurethane Foam and Structure * Front Upholstered Dual Curve Backrest (19"w x 24"h)   Arms:  Midnight Black / Light Grey [G]  **Options:**   * tCentric Armrest Height & Lateral [TCL / TCLG] * tCentric Armrest Height & Swivel [TC360 / TC360G] * tCentric Armrest Height, Lateral & Swivel [TCL360 / TCL360G]   Seat:   * Dual Density Molded Polyurethane Foam * Eight Ply Hardwood Seat Structure Seat Pan (20”w x 19”d) * Tailored Upholstery on Seat Pan   **Options:**   * Extra Small (17 ½”w x 15 ½d) [XSS] * Small Seat (18 ½”w x 17”d) [SS] * Standard Seat (20”w x 19”d) [LS] * Plus Size (22”w x 19”d) [PS] * Extra Long Seat (20”w x 21”d) [XLS] * Triple Density Foam (adds ¼” to seat width & depth) [TDF] * Non-Tailored Seat Pan [NTS]   Pneumatic Lift (Seat Height): Midnight Black / Light Grey   * 200 mm Pneumatic Lift (23 ½” – 30 ¾")   **Options:**  *Midnight Black / Light Grey [G]*   * 157 mm Pneumatic Lift (19 ¾” - 25 ½”) [157MM/G157MM] * 267 mm Pneumatic Lift (25 ¾” – 35 ¾”) [267MM/G267MM] | Counter Height Mechanism:   * Independent Back Angle Adjustment * Fixed Seat * Seat Height   Base/Glides/Casters:  *Midnight Black/Light Grey*   * 26" Glass Reinforced Nylon Mid Profile Base * 20” Diameter Aluminum, Height Adjustable Footring (1 ¾” foot platform) * 1 ¼” Glides   **Options:**   * Lock-on Urethane Casters [LON] * Lock-off Urethane Casters [LOF] * Single Wheel Nylon Casters [SW] * Single Wheel Urethane Casters [SWU] * Dual Wheel Nylon Casters [NC] * Dual Wheel Urethane Casters [UC] * 2 ¼” Glides [2G]   Additional Options:   * Modified Multi Tilt Mechanism [MT] * Dedicated Task 2 Mechanism [DT2]   Measurements:  Boxed Weight / Size   * 56 lbs. / 11.7 cu. ft.   \*Mixing of Midnight Black & Light Grey components is not an option. |