airCentric™2

|  |  |
| --- | --- |
| Counter Height\* | Midnight Black [air2-CH/air2S-CH] |
| Light Grey [air2-CHG/air2S-CHG] |
|  |
| Backrest:Midnight Black / Light Grey* 5" Patented Back Height Adjustment System
* Plastic Back Cap with Airflow Vents [air2]
* Solid Back Cap [air2S]
* Proprietary Airflow Molded Polyurethane Foam and Structure
* Front Upholstered Dual Curve Backrest (19"w x 24"h)

Arms: Midnight Black / Light Grey [G] **Options:*** tCentric Armrest Height & Lateral [TCL / TCLG]
* tCentric Armrest Height & Swivel [TC360 / TC360G]
* tCentric Armrest Height, Lateral & Swivel [TCL360 / TCL360G]

Seat:* Dual Density Molded Polyurethane Foam
* Eight Ply Hardwood Seat Structure Seat Pan (20”w x 19”d)
* Tailored Upholstery on Seat Pan

**Options:*** Extra Small (17 ½”w x 15 ½d) [XSS]
* Small Seat (18 ½”w x 17”d) [SS]
* Standard Seat (20”w x 19”d) [LS]
* Plus Size (22”w x 19”d) [PS]
* Extra Long Seat (20”w x 21”d) [XLS]
* Triple Density Foam (adds ¼” to seat width & depth) [TDF]
* Non-Tailored Seat Pan [NTS]

Pneumatic Lift (Seat Height):Midnight Black / Light Grey* 200 mm Pneumatic Lift (23 ½” – 30 ¾")

**Options:***Midnight Black / Light Grey [G]** 157 mm Pneumatic Lift (19 ¾” - 25 ½”) [157MM/G157MM]
* 267 mm Pneumatic Lift (25 ¾” – 35 ¾”) [267MM/G267MM]
 | Counter Height Mechanism:* Independent Back Angle Adjustment
* Fixed Seat
* Seat Height

Base/Glides/Casters:*Midnight Black/Light Grey** 26" Glass Reinforced Nylon Mid Profile Base
* 20” Diameter Aluminum, Height Adjustable Footring (1 ¾” foot platform)
* 1 ¼” Glides

**Options:*** Lock-on Urethane Casters [LON]
* Lock-off Urethane Casters [LOF]
* Single Wheel Nylon Casters [SW]
* Single Wheel Urethane Casters [SWU]
* Dual Wheel Nylon Casters [NC]
* Dual Wheel Urethane Casters [UC]
* 2 ¼” Glides [2G]

Additional Options:* Modified Multi Tilt Mechanism [MT]
* Dedicated Task 2 Mechanism [DT2]

Measurements:Boxed Weight / Size* 56 lbs. / 11.7 cu. ft.

\*Mixing of Midnight Black & Light Grey components is not an option. |