airCentric™2

|  |  |
| --- | --- |
| Knee Tilt | Midnight Black [air2-KT/air2S-KT] |
|  | |
| Backrest:  Midnight Black   * 5" Patented Back Height Adjustment System * Plastic Back Cap with Airflow Vents [air2] * Solid Back Cap [air2S] * Proprietary Airflow Molded Polyurethane Foam and Structure * Front Upholstered Dual Curve Backrest (19"w x 24"h)   Arms:  Midnight Black  **Options:**   * tCentric Armrest Height & Lateral [TCL] * tCentric Armrest Height & Swivel [TC360] * tCentric Armrest Height, Lateral & Swivel [TCL360]   Seat:   * Dual Density Molded Polyurethane Foam * Eight Ply Hardwood Seat Structure Seat Pan (20”w x 19”d) * Tailored Upholstery on Seat Pan   **Options:**   * Extra Small (17 ½”w x 15 ½d) [XSS] * Small Seat (18 ½”w x 17”d) [SS] * Standard Seat (20”w x 19”d) [LS] * Plus Size (22”w x 19”d) [PS] * Extra Long Seat (20”w x 21”d) [XLS] * Energy Absorbent Memory Foam [EA] * Triple Density Foam (adds ¼” to seat width & depth) [TDF] * Non-Tailored Seat Pan [NTS]   Pneumatic Lift (Seat Height):   * 125 mm Pneumatic Lift (18" – 23")   **Options:**   * 80 mm Pneumatic Lift (15 ¼”-18 ¼”) [80MM] (only available with 26” Glass Reinforced Nylon Base) * 100 mm Pneumatic Lift (15 ½”-19”) [100MM] * 140 mm Pneumatic Lift (19”-24 ½”) [140MM] | Knee Tilt Mechanism:   * Infinite Lock Free Float * Back Angle Adjustment * Adjustable Spring Tension * 2 ½” Depth Adjustable Seat Slider   Base/Glides/Casters:   * 25" Glass Reinforced Nylon High Profile Base * 5 Dual Wheel Nylon Carpet Casters   **Options:**   * 26” Glass Reinforced Nylon Base [26NB] * 26” Glass Reinforce Nylon Mid-Profile Base [26MP] * 26” Polished Aluminum Base [26PB] * Chrome Accent Casters [CAC] * Dual Wheel Urethane Casters [UC] * Single Wheel Casters [SW] * Single Wheel Urethane Casters [SWU] * 2 ¼” Glides [2G]   Additional Options:   * Air Lumbar [AL] * Air Thoracic [AT] * Tailored Adjustable Headrest [AHR]   Measurements:  Boxed Weight / Size   * 56 lbs. / 11.7 cu. ft. |