e500™ Series

|  |  |
| --- | --- |
| E500 Mechanism [e500] |  |
|  | |
| Backrest:   * Fully Upholstered Dual Curve Backrest (21"w x 26"h) * Bolstered Fabricated Polyurethane Foam * Fixed Height   Arms:   * 9 ½" e500 Fixed Height Armrests [E50010]   **Options:**   * 12" e500 Fixed Height Armrests [E50012]   Seat:   * Heavy Duty Polyurethane Foam * Eleven Ply Hardwood Seat Structure * Fully Upholstered Seat Pan (22"w x 21"d) [24CPS]   **Options:**   * Large Heavy Duty Seat (24"w x 21"d) [E5LSHD] * Extra Wide Seat (26"w x 21"d) [E5XW]   Pneumatic Lift (Seat Height):   * 100 mm (500 lb.) Super Heavy Duty Lift (16" - 20") [100MMHD]   e500 Mechanism:   * Single Position Tilt Lock * Adjustable Spring Tension * Synchro 2:1 Ratio * Height Adjustable   Base/Glides/Casters   * 6 Legged Steel Base, 26" Caster Center * 75mm Heavy Duty Multi Surface Casters   Additional Options:   * Air Lumbar [AL] * Air Thoracic [AT] * Air Thoracic and Air Lumbar [ATL] * Adjustable Headrest [24AHR]   Measurements:  Boxed Weight / Size   * 71 lbs. / 11.7 cu. ft. |  |