ergoForce High BackPlus Size Multi Tilt [eForce-HB-PLUS-350MT]

|  |  |
| --- | --- |
| Backrest* 5" Patented Back Height Adjustment System
* Abrasion resistant strip on bottom of backrest 7” high
* Fully Upholstered Dual Curved Backrest (19”w x 26”h)
* Heavy Duty Back Bar Support
* Molded Polyurethane Foam

 Arms* [Click here](http://ergocentric.com/resource/arms) to view options

Seat* Abrasion resistant strip on back of seat
* Eight Ply Hardwood Seat Structure
* High Resilient Polyurethane Foam
* Seat Pan 22" wide by 19" deep

**Options:*** Extra Large Seat (22"Wx21"D) [SS]
* Triple Density Foam Seat (Adds 1/4" to seat width and depth) [TDF]
* Tailored Upholstery on Seat Pan [TS]

Heavy Duty Multi Tilt Mechanism* Forward Tilt Lock Out
* Adjustable Spring Tension
* Infinite Lock Free Float
* 2.5" Depth Adjustable Seat Slider
* Back Angle Adjustment

 Pneumatic Lift (Seat Height)* 125 mm Pneumatic Lift Heavy Duty

(seat height -17.5"-22.5")**Options:*** 80 mm Heavy Duty pneumatic lift (17"-20") [80mm]
* 100 mm Heavy Duty pneumatic lift (17.25-20.75") [100mm]
* 140 mm Heavy Duty pneumatic lift (18"-23.5") [140mm]
 | Base/Glides/Casters* 27" Hercules Glass Reinforced Nylon Base
* 5 Dual Wheel Nylon Carpet Casters

 **Options:*** 2 1/4" Glides [2G]
* Chrome Accent Casters [CAC]
* Single Wheel Casters [SW]
* Single Wheel Urethane Casters [SWU]
* Urethane Casters [UC]

Additional Options* Air Lumbar [AL]
* Air Thoracic [AT]
* Air Thoracic and Air Lumbar [ATL]
* Adjustable Headrest [AHR]
* Heavy Duty Control (Task Intensive) [TI]

 |