ergoForce™ High BackSynchro Glide [eForce-HB-SG]

|  |  |
| --- | --- |
| Backrest   * Fully Upholstered Dual Curve Backrest (19”w x 26”h) * 5” Patented Back Height Adjustment System * Abrasion resistant strip on bottom of backrest   Arms   * [Click here](http://ergocentric.com/resource/arms) to view options   Seat   * Abrasion resistant strip on back of seat * Eight Ply Hardwood Seat Structure * High Resilient Polyurethane Foam * Seat Pan 20”w x 19”d   **Options:**   * Memory Foam Seat [EA] * Extra Long Seat (20”w x 21”d) [XLS] * Small Seat (18.5”w x 17”d) [SS] * Triple Density Foam Seat (Adds ¼” to seat width and depth) [TDF] * Tailored Upholstery on Seat Pan [TS]   Synchro Glide Mechanism   * 2.5” Depth Adjustable Seat Slider * Adjustable Spring Tension * Infinite Lock Free Float * Independent Back Angle Adjustment * Seat Tilt lock out * Synchro 2:1 Ratio   Pneumatic Lift (Seat Height)   * 125 mm Pneumatic Lift (16" – 21")   **Options:**   * 80 mm Pneumatic Lift (15.25”-18.25”) [80mm] * 100 mm Pneumatic Lift (15.5”-19”) [100mm] * 140 mm Pneumatic Lift (17”-22.5”) [140mm] | Base/Glides/Casters   * 26” Glass Reinforced Nylon Base * 5 Dual Wheel Nylon Carpet Casters   **Options:**   * 2 ¼” Glides [2G] * Chrome Accent Casters [CAC] * 26” Polished Aluminum Base [PB] * Single Wheel Casters [SW] * Single Wheel Urethane Casters [SWU] * Urethane Casters [UC]   Additional Options   * Air Lumbar [AL] * Air Thoracic [AT] * Air Thoracic and Air Lumbar [ATL] * Adjustable Headrest [AHR] |