ergoForce™ Mid BackDedicated Task [eForce-MB-DT]

|  |  |
| --- | --- |
| Backrest* Fully Upholstered Dual Curve Backrest (15.5”w x 19”h)
* 5” Patented Back Height Adjustment System
* Abrasion resistant strip on bottom of backrest

Arms* [Click here](http://ergocentric.com/resource/arms) to view options

Seat* Abrasion resistant strip on back of seat
* Eight Ply Hardwood Seat Structure
* High Resilient Polyurethane Foam
* Seat Pan 20”w x 19”d

**Options:*** 1.5” Seat Slider when used with an Extra Small Seat [XSS]
* Memory Foam Seat [EA]
* Extra Long Seat (20”w x 21”d) [XLS]
* Extra Small Seat (17.5” w x 15.5”(Recommended with TATA arm option) [XSS]
* 2.5” Seat Slider (Adds 1 ½” to seat height [SSLF]
* Small Seat (18.5”w x 17”d) [SS]
* Triple Density Foam Seat (Adds ¼” to seat width and depth) [TDF]
* Tailored Upholstery on Seat Pan [TS]

Dedicated Task Mechanism* Independent Back Angle Adjustment
* Seat Angle Adjustment
* Seat Height

Pneumatic Lift (Seat Height)* 125 mm Pneumatic Lift (16.5" – 21.5")

**Options:*** 80 mm Pneumatic Lift (15.75”-18.75”) [80mm]
* 100 mm Pneumatic Lift (16”-19.5”) [100mm]
* 140 mm Pneumatic Lift (17.5”-23”) [140mm]
* 157 mm Pneumatic Lift (17.25 “ – 23.25”) [157]
 | * 200 mm Pneumatic Lift (21.5”-28.5”) [200mm]
* 267 mm Pneumatic Lift (24“ – 34”) [267]

Base/Glides/Casters* 26” Glass Reinforced Nylon Base
* 5 Dual Wheel Nylon Carpet Casters

**Options:*** 2 ¼” Glides [2G]
* Chrome Accent Casters [CAC]
* Single Wheel Casters [SW]
* Single Wheel Urethane Casters [SWU]
* Urethane Casters [UC]

Additional Options* 20” Diameter Height Adjustable Footring (for use as foot rest only) [20FR]
* Air Lumbar [AL]
* Air Thoracic [AT]
* Air Thoracic and Air Lumbar [ATL]
* Adjustable Headrest [AHR]

  |