ergoForce™ Mid BackDedicated Task [eForce-MB-DT]

|  |  |
| --- | --- |
| Backrest   * Fully Upholstered Dual Curve Backrest (15.5”w x 19”h) * 5” Patented Back Height Adjustment System * Abrasion resistant strip on bottom of backrest   Arms   * [Click here](http://ergocentric.com/resource/arms) to view options   Seat   * Abrasion resistant strip on back of seat * Eight Ply Hardwood Seat Structure * High Resilient Polyurethane Foam * Seat Pan 20”w x 19”d   **Options:**   * 1.5” Seat Slider when used with an Extra Small Seat [XSS] * Memory Foam Seat [EA] * Extra Long Seat (20”w x 21”d) [XLS] * Extra Small Seat (17.5” w x 15.5” (Recommended with TATA arm option) [XSS] * 2.5” Seat Slider (Adds 1 ½” to seat height [SSLF] * Small Seat (18.5”w x 17”d) [SS] * Triple Density Foam Seat (Adds ¼” to seat width and depth) [TDF] * Tailored Upholstery on Seat Pan [TS]   Dedicated Task Mechanism   * Independent Back Angle Adjustment * Seat Angle Adjustment * Seat Height   Pneumatic Lift (Seat Height)   * 125 mm Pneumatic Lift (16.5" – 21.5")   **Options:**   * 80 mm Pneumatic Lift (15.75”-18.75”) [80mm] * 100 mm Pneumatic Lift (16”-19.5”) [100mm] * 140 mm Pneumatic Lift (17.5”-23”) [140mm] * 157 mm Pneumatic Lift (17.25 “ – 23.25”) [157] | * 200 mm Pneumatic Lift (21.5”-28.5”) [200mm] * 267 mm Pneumatic Lift (24“ – 34”) [267]   Base/Glides/Casters   * 26” Glass Reinforced Nylon Base * 5 Dual Wheel Nylon Carpet Casters   **Options:**   * 2 ¼” Glides [2G] * Chrome Accent Casters [CAC] * Single Wheel Casters [SW] * Single Wheel Urethane Casters [SWU] * Urethane Casters [UC]   Additional Options   * 20” Diameter Height Adjustable Footring (for use as foot rest only) [20FR] * Air Lumbar [AL] * Air Thoracic [AT] * Air Thoracic and Air Lumbar [ATL] * Adjustable Headrest [AHR] |