geoCentric™

|  |  |
| --- | --- |
| Dedicated Task Series | Mid Back [geo-MB-DT2] |
|  | |
| Backrest   * 5" Patented Back Height Adjustment System * Fully Upholstered Dual Curve Backrest (17”w x 19”h)   Arms  **Options:**   * 4” Height Adjustable Arm [4ATAOT] * 3” Height Adjustable Arm [3ATAOT]   Seat   * Dual Density Molded Polyurethane Foam * Eight Ply Hardwood Seat Structure Seat Pan (20”w x 19”d) * Tailored Upholstery on Seat Pan   **Options:**   * Extra Small (17 ½”w x 15 ½d) [XSS] * Small Seat (18 ½”w x 17”d) [SS] * Standard Seat (20”w x 19”d) [LS] * Plus Size (22”w x 19”d) [PS] * Extra Long Seat (20”w x 21”d) [XLS] * Energy Absorbent Memory Foam [EA] * Triple Density Foam (adds ¼” to seat width & depth) [TDF] * 2 ½” Seat Slider (adds 1 ½” to seat height) [SSLF] * Tailored Upholstery on Seat Pan [TS] * Non-Tailored Seat Pan [NTS]   Pneumatic Lift (Seat Height)   * 125 mmLT Pneumatic Lift (15 ½” – 20 ½”)   **Options:**   * 70 mm Pneumatic Lift (15”- 17 ¾”) [70MM] * 80 mm Pneumatic Lift (15 ¾” – 18 ½”) [80MM] * 100 mm Pneumatic Lift (16 ¼”-20”) [100MM] * 140 mm Pneumatic Lift (17 ½”- 23 ¾”) [140MM] * 157 mm Pneumatic Lift (19 ¾” – 25 ½”) [157MM] * 200 mm Pneumatic Lift (23 ½” – 30 ¾”) Glides recommended [200MM] * 267 mm Pneumatic Lift (25 ¾” – 35 ¾”) Glides recommended [267MM] | Dedicated Task 2 Mechanism   * Independent Back Angle Adjustment * Seat Angle Adjustment * Seat Height   Base/Glides/Casters   * 26" Glass Reinforced Nylon Mid Profile Base * 5 Dual Wheel Nylon Casters   **Options:**   * Chrome Accent Casters [CAC] * Dual Wheel Urethane Casters [UC] * Single Wheel Casters [SW] * Single Wheel Urethane Casters [SWU] * 2 ¼” Glides [2G]   Additional Options   * Air Lumbar [AL] * Air Thoracic [AT] * Adjustable Headrest [AHR] * Thoracic Back Support [THB] * Plastic Back Cap – Fabric [PBCMBF] * 20” Diameter Height Adjustable Footring (Used as a footrest on 200mm and 267mm lifts only)   Measurements  Boxed Weight / Size   * 42 lbs. / 6.7 cu. ft. |