geoCentric™

|  |  |
| --- | --- |
| Synchro Glide Series | Extra High Back [geo-XHB-SG] |
|  | |
| Backrest:   * 5" Patented Back Height Adjustment System * Fully Upholstered Dual Curve Backrest (19”w x 34”h)   Arms:  **Options:**   * 4” Height Adjustable Arm [4ATAOT] * 3” Height Adjustable Arm [3ATAOT] * 4” Height Adjustable Swivel Arm [SWV]   Seat:   * Dual Density Molded Polyurethane Foam * Eight Ply Hardwood Seat Structure Seat Pan (20”w x 19”d) * Tailored Upholstery on Seat Pan   **Options:**   * Extra Small (17 ½”w x 15 ½d) [XSS] * Small Seat (18 ½”w x 17”d) [SS] * Standard Seat (20”w x 19”d) [LS] * Plus Size (22”w x 19”d) [PS] * Extra Long Seat (20”w x 21”d) [XLS] * Energy Absorbent Memory Foam [EA] * Triple Density Foam (adds ¼” to seat width & depth) [TDF] * Non-Tailored Seat Pan [NTS]   Pneumatic Lift (Seat Height):   * 125 mmLT Pneumatic Lift (17 ½” – 22 ¼”)   **Options:**   * 70 mm Pneumatic Lift (17”- 19 ¾”) [70MM] * 80 mm Pneumatic Lift (17 ¾” – 20 ¾”) [80MM] * 100 mm Pneumatic Lift (18 ½”-22”) [100MM] * 140 mm Pneumatic Lift (19 ½”- 25”) [140MM]   Synchro Glide Mechanism:   * Seat Tilt Lock Out * Free Float * Independent Back Angle Adjustment * Synchro 2:1 ratio * Adjustable Spring Tension * 2 ½” Depth Adjustable Seat Slider | Base/Glides/Casters:   * 26" Glass Reinforced Nylon Mid Profile Base * 5 Dual Wheel Nylon Casters   **Options:**   * 26” Polished Aluminum Mid Profile Base [PMB] * Chrome Accent Casters [CAC] * Dual Wheel Urethane Casters [UC] * Single Wheel Casters [SW] * Single Wheel Urethane Casters [SWU] * 2 ¼” Glides [2G]   Additional Options:   * Air Lumbar [AL] * Air Thoracic [AT] * Air Thoracic and Air Lumbar [ATL] * Neck Support [NNS]   Measurements:  Boxed Weight / Size   * 63 lbs. / 11.7 cu. ft. |