geoCentric™

|  |  |
| --- | --- |
| Dedicated Task Series | Extra Tall Back [geo-XTB-DT2] |
|  |
| Backrest:* 5" Patented Back Height Adjustment System
* Fully Upholstered Dual Curve Backrest (19”w x 25”h)

Arms:**Options:*** 4” Height Adjustable Arm [4ATAOT]
* 3” Height Adjustable Arm [3ATAOT]

Seat:* Dual Density Molded Polyurethane Foam
* Eight Ply Hardwood Seat Structure Seat Pan (20”w x 19”d)
* Tailored Upholstery on Seat Pan

**Options:*** Extra Small (17 ½”w x 15 ½d) [XSS]
* Small Seat (18 ½”w x 17”d) [SS]
* Standard Seat (20”w x 19”d) [LS]
* Plus Size (22”w x 19”d) [PS]
* Extra Long Seat (20”w x 21”d) [XLS]
* Energy Absorbent Memory Foam [EA]
* Triple Density Foam (adds ¼” to seat width & depth) [TDF]
* 2 ½” Seat Slider (adds 1 ½” to seat height)
* Tailored Upholstery on Seat Pan [TS]
* Non-Tailored Seat Pan [NTS]

Pneumatic Lift (Seat Height):* 125 mmLT Pneumatic Lift (15 ½” – 20 ½”)

**Options:***Midnight Black / Light Grey [G]** 70 mm Pneumatic Lift (15”- 17 ¾”) [70MM]
* 80 mm Pneumatic Lift (15 ¾” – 18 ½”) [80MM]
* 100 mm Pneumatic Lift (16 ¼”-20”) [100MM]
* 140 mm Pneumatic Lift (17 ½”- 23 ¾”) [140MM]
* 157 mm Pneumatic Lift (19 ¾” – 25 ½”) [157MM]
* 200 mm Pneumatic Lift (23 ½” – 30 ¾”) [200MM]
 | Dedicated Task 2 Mechanism:* Independent Back Angle Adjustment
* Seat Angle Adjustment
* Seat Height

Base/Glides/Casters: * 26" Glass Reinforced Nylon Mid Profile Base
* 5 Dual Wheel Nylon Casters

**Options:*** Chrome Accent Casters [CAC]
* Dual Wheel Urethane Casters [UC]
* Single Wheel Casters [SW]
* Single Wheel Urethane Casters [SWU]
* 2 ¼” Glides [2G]

Additional Options:* Air Lumbar [AL]
* Air Thoracic [AT]
* Air Thoracic and Air Lumbar [ATL]
* Adjustable Headrest [AHR]
* Thoracic Back Support [THB]
* 20” Diameter Height Adjustable Footring (Used as a footrest on 200mm and 267mm lifts only)

Measurements:Boxed Weight / Size * 52 lbs./11.7 cu. ft.
 |