tCentric Hybrid™

|  |  |  |
| --- | --- | --- |
| All Mesh – Counter Height\* | | Midnight Black [t-MBMESH-CH] |
| Light Grey [t-LGMESH-CHG] |
| Backrest:  Midnight Black / Light Grey   * 5" Patented Back Height Adjustment System * Dual Curve Mesh Backrest (19"w x 25"h)   Arms:  Midnight Black / Light Grey [G]  **Options:**   * tCentric Armrest Height & Lateral [TCL / TCLG] * tCentric Armrest Height & Swivel [TC360 / TC360G] * tCentric Armrest Height, Lateral & Swivel [TCL360 / TCL360G]   Seat: Midnight Black / Light Grey   * Airless Cushion Technology * Mesh Seat with 30% Glass Filled Nylon Frame (21”w x 18 ½”d)   **Options:**  *Midnight Black [MB] / Light Grey [G]*   * Small Mesh Seat (20”w x 16 ½”d) [TMBMSS / TLGMSS] * Extra Long Mesh Seat (21”w x 20 ½”d) [TMBMXLS / TLGMXLS]   Counter Height Mechanism:  Midnight Black / Light Grey   * Independent Back Angle Adjustment * Fixed Seat * Seat Height   **Options:**  *Midnight Black*   * Multi-Tilt (with height and back angle adjustment) [MT] * Dedicated Task 2 Mechanism [DT2]   Pneumatic Lift (Seat Height): Midnight Black / Light Grey   * 200 mm Pneumatic Lift (24 ¾" - 32")   **Options:**  *Midnight Black / Light Grey [G]*   * 157 mm Pneumatic Lift (24 ¾” – 32”) [157MM/G157MM] * 267 mm Pneumatic Lift (27”-37”) [267MM/G267MM]   Measurements/Overall Dimensions:   * Boxed Weight/Size: 56 lbs. / 6.7 cu.ft. | Base/Footring/Glides/Casters:   * 26" Glass Reinforced Nylon Mid-Profile Base *(Midnight Black / Light Grey)* * Aluminum, Height Adjustable Footring (20” Diameter, 1 ¾” Thick Foot Platform) * 1 ¼” Glides   **Options:**   * Lock-on Urethane Casters [LON] * Lock-off Urethane Casters [LOF] * Dual Wheel Urethane Casters [UC] * Dual Wheel Nylon Casters [NC] * Single Wheel Urethane Casters [SWU] * Single Wheel Nylon Casters [SW] * 2 ¼” Glides   Additional Options:  Midnight Black / Light Grey [G]   * tCentric Lumbar Support [TLS / TLSG] * tCentric Lumbar Support with Air Lumbar (pump) [TLSAL / TLSALG] * Adjustable Headrest [AHR / AHRG]   Mesh Material:  Both the tCentric Hybrid seat and backrest are made from elastomeric mesh with fill yarns made from polyester.  When stretched, this material yields excellent load-bearing properties and resiliency, showing less than 5% load-bearing loss when tested according to BIFMA standards.  To clean use mild household or hospital detergents.  \*Mixing of Midnight Black & Light Grey components is not an option. | |