tCentric Hybrid™

|  |  |
| --- | --- |
| All Mesh – Counter Height\* | Midnight Black [t-MBMESH-CH] |
| Light Grey [t-LGMESH-CHG] |
| Backrest:Midnight Black / Light Grey* 5" Patented Back Height Adjustment System
* Dual Curve Mesh Backrest (19"w x 25"h)

Arms: Midnight Black / Light Grey [G]**Options:*** tCentric Armrest Height & Lateral [TCL / TCLG]
* tCentric Armrest Height & Swivel [TC360 / TC360G]
* tCentric Armrest Height, Lateral & Swivel [TCL360 / TCL360G]

Seat:Midnight Black / Light Grey* Airless Cushion Technology
* Mesh Seat with 30% Glass Filled Nylon Frame (21”w x 18 ½”d)

**Options:***Midnight Black [MB] / Light Grey [G]** Small Mesh Seat (20”w x 16 ½”d) [TMBMSS / TLGMSS]
* Extra Long Mesh Seat (21”w x 20 ½”d) [TMBMXLS / TLGMXLS]

Counter Height Mechanism:Midnight Black / Light Grey* Independent Back Angle Adjustment
* Fixed Seat
* Seat Height

**Options:***Midnight Black* * Multi-Tilt (with height and back angle adjustment) [MT]
* Dedicated Task 2 Mechanism [DT2]

Pneumatic Lift (Seat Height):Midnight Black / Light Grey * 200 mm Pneumatic Lift (24 ¾" - 32")

**Options:***Midnight Black / Light Grey [G]** 157 mm Pneumatic Lift (24 ¾” – 32”) [157MM/G157MM]
* 267 mm Pneumatic Lift (27”-37”) [267MM/G267MM]

Measurements/Overall Dimensions:* Boxed Weight/Size: 56 lbs. / 6.7 cu.ft.
 | Base/Footring/Glides/Casters:* 26" Glass Reinforced Nylon Mid-Profile Base *(Midnight Black / Light Grey)*
* Aluminum, Height Adjustable Footring (20” Diameter, 1 ¾” Thick Foot Platform)
* 1 ¼” Glides

**Options:*** Lock-on Urethane Casters [LON]
* Lock-off Urethane Casters [LOF]
* Dual Wheel Urethane Casters [UC]
* Dual Wheel Nylon Casters [NC]
* Single Wheel Urethane Casters [SWU]
* Single Wheel Nylon Casters [SW]
* 2 ¼” Glides

Additional Options: Midnight Black / Light Grey [G]* tCentric Lumbar Support [TLS / TLSG]
* tCentric Lumbar Support with Air Lumbar (pump) [TLSAL / TLSALG]
* Adjustable Headrest [AHR / AHRG]

Mesh Material:Both the tCentric Hybrid seat and backrest are made from elastomeric mesh with fill yarns made from polyester. When stretched, this material yields excellent load-bearing properties and resiliency, showing less than 5% load-bearing loss when tested according to BIFMA standards.To clean use mild household or hospital detergents.\*Mixing of Midnight Black & Light Grey components is not an option. |