ergoCentric3-in-1 Sit Stand [3 in 1 Sit Stand]

|  |  |  |  |
| --- | --- | --- | --- |
| Backrest* Fully upholstered backrest (14"w x 10"h)
* 4" of back height adjustment

Seat* Upholstered seat with dual density molded polyurethane Foam with 5" ergoCentric+Guard™ No-Slip Strip
* Seat pan 17.5" wide by 15.5" deep

|  |  |
| --- | --- |
|   | *Options*: > 3-in-1 Large seat pan (18.5"w x 17"d) [SS] |

Dedicated Task Control 2* 1 Lever for both seat and back angle adjustment
* Back height adjustment
* Back pivot
* Seat height

Pneumatic Lift (Seat Height)* 200mm Knurled dual height adjustment system (seat height 7.5" of adjustment between 19.25"- 35.5")

Base/Glides/Casters* 22" Chrome 22 base has an 18" oval tube foot ring built in for durability
* 2 x 2 ¼" Dual wheel nylon casters and 3 x 2 ¼" glides
* Options:
* 5 x 2 ¼" Glides [2G]
* 2 x Urethane casters and 2 x 2 ¼" glides [2UC32G]

Additional Options* 3-in-1 High Back (17"w x 15"h) [3N1HB]
* Cal. 133 [Cal133]
 |  |