iCentric™Mesh Executive Boardroom [I-MESH-EXBR]

|  |  |
| --- | --- |
| Backrest   * Available in 3 Color Options: Black (standard), Dark Chocolate and Silver (see options section) * Polyester and monofilament knit sock with a horizontal band detail * Welded steel tubular frame 21” w x 24” h - Tapered width   Seat   * Eight Ply Hardwood Seat Structure * High Resilient Polyurethane Foam * Matching Fabric Seat Options to Backrest Colors Available (see option section) * Seat Pan 20.5” wide by 18.5” deep   **Available Backrest Mesh Color Options:**   * Black with Black Horizontal Band Detail Standard [VN7209B] * Dark Chocolate with Black Horizontal Band Detail [VN4129B] * Silver with Black Horizontal Band Detail [VN7273B]   **Matching Seat Upholstery Options:**   * Open House Asteroid Grade 1 [OH2053] * Open House Coffee Bean Grade 1 [OH2083] * Open House Onyx Grade 1 [OH2016]   **Matching Seat Mesh Options Without Horizontal Band Detail:**   * Black Grade 2 [VN7209S] * Dark Chocolate Grade 2 [VN4129S] * Silver Grade 2 [VN7273S]   Executive Boardroom Control   * 5 Position Tilt Lock * Adjustable Spring Tension * Free Float * Seat Height | Pneumatic Lift (Seat Height)   * 125 mm Pneumatic Lift (16.5" – 21.5")   **Options:**   * 80 mm Pneumatic Lift (only available with 26” glass reinforced nylon base) (15.75”-18.75”) [80mm] * 100 mm Pneumatic Lift (16”-19.5”) [100mm] * 140 mm Pneumatic Lift (17.5”-23”) [140mm]   Base/Glides/Casters   * 25” Glass Reinforced Nylon High Profile Base * 5 Dual Wheel Nylon Carpet Casters * **Options:** * 2 ¼” Glides [2G] * 26” Glass Reinforced Nylon Base [26NB] * Chrome Accent Casters[CAC] * 26” Polished Aluminum Base [PB] * 26” Polished Aluminum High Profile Base [PB2] * Single Wheel Casters [SW] * Single Wheel Urethane Casters [SWU] * Urethane Casters [UC]   Additional Options   * Accent Mesh [ACCENT] * Executive Mechanism [EXEC] |