tCentric Hybrid™Accent [t-A]

|  |  |
| --- | --- |
| Backrest* 5" Patented Back Height Adjustment SystemDual Curve Mesh Backrest (19"w x 25"h)

Arms* [Click here](http://ergocentric.com/resource/arms) to view options

Seat* Eight Ply Hardwood Seat Structure
* Seat Pan 20" wide by 19" deep
* Dual Density Molded Polyurethane

Accent Mechanism* Adjustable Spring Tension
* Seat Height
* Single Lock Free Float

Pneumatic Lift (Seat Height)* 125 mm Pneumatic Lift (19" - 24")

**Options:*** 80 mm Pneumatic Lift (18"-21") [80mm]
* 100 mm Pneumatic Lift (18.25”-21.75” [100mm]
* 100 mm Pneumatic Lift Chrome (18”-21”) [100mmCH]
* 125 mm Pneumatic Lift Chrome (18.25”-21.75”) [125mmCH]
* 140 mm Pneumatic Lift (20”-25.5”) [140mm]
* 140 mm Pneumatic Lift Chrome (20” – 25.5”) [140mmCH]
 | Base/Glides/Casters* 26" Glass Reinforced Nylon High Profile Base 2
* 5 Dual Wheel Nylon Carpet Casters 2

**Options:*** Chrome Accent Casters [CAC]
* 26" Polished Aluminum High Profile Base [PB2]
* Urethane Caster [UC2]

Additional Options* Adjustable Headrest [AHR]
* CooltoTouch Lumbar Support (12"w x 6"h) [TLS]
* CooltoTouch Lumbar Support with Air Lumbar [TLSAL]

Measurements / Overall DimensionsBoxed Weight/Size (56 lbs./11.7 cu.ft) |