ecoCentric Stacker With Arms [eco-STACKER-A]

|  |  |
| --- | --- |
| Backrest* Backrest 20" wide by 12.5" high
* Dual curve plastic backrest
* Handle in back for easy movement
* Unique scalloped indentations for the spine provides additional comfort

**Options:*** Upholstered Back [UPHB]

Arms* Tablet Arm

**Options:*** Padded Nytek Arm Cover (Permanent Cover) [PNY]

Seat* 17" Seat Height
* Dual Curve Waterfall Plastic Seat in Black
* Seat Pan 18" wide by 18.5" deep
* Unique Scalloped Indentations for the Seat Bones

**Options:*** Grey Package (Includes grey seat, backrest and arm caps) [ECOGP]
* Upholstered Seat [UPHS]
 | Base/Glides/Casters**Options:*** Nylon Stacker Casters [NSC]
* Urethane Stacker Casters [USC]
* Metal Sled base option with glass reinforced nylon glides (chair does not stack with sled base option) [SLED]

Frame* 14 Gauge, 7/8" Steel Tube Frame
* Black Textured Semi-Gloss Powder Coat Paint
* Glass filled nylon arms (black)
* Kick Back Legs for Stability with Durable Custom Glides

**Options*** Chrome frame (CF)
* Wall saver frame (WSF)

Additional Options* Grey Arm Cap [GAC]
* Grey Plastic Backrest (20”w x 12.5”d) [PLABG]
* Grey Plastic Seat (18”w x 18.5”d) [PLASG]
* Ganging clips (set of 2) chair with arms [GC]
 |