ecoCentric Stacker Armless [eco-STACKER]

|  |  |
| --- | --- |
| Backrest   * Backrest 20" wide by 12.5" high * Dual curve plastic backrest * Handle in back for easy movement * Unique scalloped indentations for the spine provides additional comfort   **Options:**   * Upholstered Back [UPHB]   Seat   * 17" Seat Height * Dual Curve Waterfall Plastic Seat in Black * Seat Pan 18" wide by 18.5" deep * Unique scalloped indentations for the seat bones   **Options:**   * Grey Package (Includes grey seat, backrest and arm caps) [ECOGP] * Upholstered Seat [UPHS] | Base/Glides/Casters  **Options:**   * Nylon Stacker Casters [NSC] * Urethane Stacker Casters [USC] * Metal Sled base option with glass reinforced nylon glides (chair does not stack with sled base option) [SLED]   Frame   * 14 Gauge, 7/8" Steel Tube Frame * Black Textured Semi-Gloss Powder Coat Paint * Kick Back Legs for Stability with Durable Custom Glides   **Options**   * Chrome frame (CF) * Wall saver frame (WSF)   Additional Options   * Grey Arm Cap [GAC] * Grey Plastic Backrest (20”w x 12.5”d) [PLABG] * Grey Plastic Seat (18”w x 18.5”d) [PLASG] * Ganging Clips (set of 2) chair with no arms [GCNA] |