geoCentric™ Tall BackSynchro Glide [geo-TB-SG]

|  |  |
| --- | --- |
| Backrest* Fully Upholstered Dual Curve Backrest (17”w x 21”h)
* 5” Patented Back Height Adjustment System

Arms* [Click here](http://ergocentric.com/resource/arms) to view options

Seat* Eight Ply Hardwood Seat Structure
* High Resilient Polyurethane Foam
* 20”w x 19”d

**Options:*** Memory Foam Seat [EA]
* Extra Long Seat (20”w x 21”d) [XLS]
* Small Seat (18.5”w x 17”d) [SS]
* Triple Density Foam Seat (Adds ¼” to seat width and depth) [TDF]
* Tailored Upholstery on Seat Pan [TS]

Synchro Glide Mechanism* 2.5” Depth Adjustable Seat Slider
* Adjustable Spring Tension
* Free Float
* Independent Back Angle Adjustment
* Seat Tilt Lock Out
* Synchro 2:1 Ratio

Pneumatic Lift (Seat Height)* 125 mm Pneumatic Lift (18" – 23")

**Options:*** 80 mm Pneumatic Lift (17.25”-20.25”) [80mm]
* 100 mm Pneumatic Lift (17.5”-21”) [100mm]
* 140 mm Pneumatic Lift (19”-24.5”) [140mm]
 | Base/Glides/Casters* 26” Glass Reinforced Nylon Base
* 5 Dual Wheel Nylon Carpet Casters

**Options:*** 2 ¼” Glides [2G]
* Chrome Accent Casters [CAC]
* 26” Polished Aluminum Base [PB]
* Single Wheel Casters [SW]
* Single Wheel Urethane Casters [SWU]
* Urethane Casters [UC]

Additional Options* Air Lumbar [AL]
* Thoracic Back Support [THB]
* Air Thoracic [AT]
* Air Thoracic and Air Lumbar [ATL]
* Adjustable Headrest [AHR]
* Cal. 133 [Cal133]

  |