airCentric™2

|  |  |
| --- | --- |
| Knee Tilt | Midnight Black [air2-KT/air2S-KT] |
|  |
| Backrest:Midnight Black* 5" Patented Back Height Adjustment System
* Plastic Back Cap with Airflow Vents [air2]
* Solid Back Cap [air2S]
* Proprietary Airflow Molded Polyurethane Foam and Structure
* Front Upholstered Dual Curve Backrest (19"w x 24"h)

Arms:Midnight Black **Options:*** tCentric Armrest Height & Lateral [TCL]
* tCentric Armrest Height & Swivel [TC360]
* tCentric Armrest Height, Lateral & Swivel [TCL360]

Seat:* Dual Density Molded Polyurethane Foam
* Eight Ply Hardwood Seat Structure Seat Pan (20”w x 19”d)
* Tailored Upholstery on Seat Pan

**Options:*** Extra Small (17 ½”w x 15 ½d) [XSS]
* Small Seat (18 ½”w x 17”d) [SS]
* Standard Seat (20”w x 19”d) [LS]
* Plus Size (22”w x 19”d) [PS]
* Extra Long Seat (20”w x 21”d) [XLS]
* Energy Absorbent Memory Foam [EA]
* Triple Density Foam (adds ¼” to seat width & depth) [TDF]
* Non-Tailored Seat Pan [NTS]

Pneumatic Lift (Seat Height):* 125 mm Pneumatic Lift (18" – 23")

**Options:*** 80 mm Pneumatic Lift (15 ¼”-18 ¼”) [80MM] (only available with 26” Glass Reinforced Nylon Base)
* 100 mm Pneumatic Lift (15 ½”-19”) [100MM]
* 140 mm Pneumatic Lift (19”-24 ½”) [140MM]
 | Knee Tilt Mechanism: * Infinite Lock Free Float
* Back Angle Adjustment
* Adjustable Spring Tension
* 2 ½” Depth Adjustable Seat Slider

Base/Glides/Casters:* 25" Glass Reinforced Nylon High Profile Base
* 5 Dual Wheel Nylon Carpet Casters

**Options:*** 26” Glass Reinforced Nylon Base [26NB]
* 26” Glass Reinforce Nylon Mid-Profile Base [26MP]
* 26” Polished Aluminum Base [26PB]
* Chrome Accent Casters [CAC]
* Dual Wheel Urethane Casters [UC]
* Single Wheel Casters [SW]
* Single Wheel Urethane Casters [SWU]
* 2 ¼” Glides [2G]

Additional Options:* Air Lumbar [AL]
* Air Thoracic [AT]
* Tailored Adjustable Headrest [AHR]

Measurements:Boxed Weight / Size* 56 lbs. / 11.7 cu. ft.
 |