geoCentric™ Extra Tall BackDedicated Task [geo-XTB-DT]

|  |  |
| --- | --- |
| Backrest   * Fully Upholstered Dual Curve Backrest (19”w x 25”h) * 5” Patented Back Height Adjustment System   Arms   * [Click here](http://ergocentric.com/resource/arms) to view options   Seat   * Eight Ply Hardwood Seat Structure * High Resilient Polyurethane Foam * 20”w x 19”d   **Options:**   * 1.5” Seat Slider when used with an Extra Small Seat [XSS] * Memory Foam Seat [EA] * Extra Long Seat (20”w x 21”d) [XLS] * Extra Small Seat (17.5”w x 15.5”d) (Recommended with TATA arm option) [XSS] * 2.5” Seat Slider (Adds 1 ½” to seat height) [SSLF] * Small Seat (18.5”w x 17”d) [SS] * Triple Density Foam Seat (Adds ¼” to seat width and depth) [TDF] * Tailored Upholstery on Seat Pan [TS]   Dedicated Task Mechanism   * Independent Back Angle Adjustment * Seat Angle Adjustment * Seat Height   Pneumatic Lift (Seat Height)   * 125 mm Pneumatic Lift (16.5" – 21")   **Options:**   * 80 mm Pneumatic Lift (15.75”-18.25”) [80mm] * 100 mm Pneumatic Lift (16.25”-20”) [100mm] * 140 mm Pneumatic Lift (17.5”-23.75”) [140mm] * 157 mm Pneumatic Lift (19.75”-25.5”) [157mm] * 200 mm Pneumatic Lift (23.5”-30.75”) [200mm] | Base/Glides/Casters   * 26” Glass Reinforced Nylon Base * 5 Dual Wheel Nylon Carpet Casters   **Options:**   * 2 ¼” Glides [2G] * Chrome Accent Casters [CAC] * Single Wheel Casters [SW] * Single Wheel Urethane Casters [SWU] * Urethane Casters [UC] * 20” Diameter Height Adjustable Footring (for use as a footrest only( [20FR]   Additional Options   * Air Lumbar [AL] * Thoracic Back Support [THB] * Air Thoracic [AT] * Air Thoracic and Air Lumbar [ATL] * Adjustable Headrest [AHR] * Cal. 133 [Cal133] |