tCentric Hybrid™

|  |  |
| --- | --- |
| Counter Height | Midnight Black [t-CH]Light Grey [t-CHG] |
| Backrest:Midnight Black / Light Grey* Dual Curve Mesh Backrest (19"w x 25"h)
* 5” Patented Back Height Adjustment System

Arms:Midnight Black / Light Grey [G]**Options:*** tCentric Armrest Height & Lateral [TCL / TCLG]
* tCentric Armrest Height & Swivel [TC360 / TC360G]
* tCentric Armrest Height, Lateral & Swivel [TCL360 / TCL360G]

Seat:* Dual Density Molded Polyurethane Foam
* Eight ply hardwood seat structure
* Tailored upholstery on seat pan (20”w x 19”d)

**Options:*** Extra Small Seat (17 ½”w x 15 ½”d) [XSS]
* Small Seat (18 ½”w x 17”d) [SS]
* Plus Size Seat (22”w x 19”d) [PS]
* Extra Long Seat (20”w x 21”d) [XLS]
* Extra Deep Seat (22”w x 21”d) [XPS]
* Energy Absorbent Memory Foam [EA]
* Triple Density Foam [TDF]
* Non-Tailored Seat Pan [NTS]

Pneumatic Lift (Seat Height):Midnight Black / Light Grey* 200 mm Pneumatic Lift (23 ½" – 30 ¾")

**Options:***Midnight Black / Light Grey [G]** 157 mm Pneumatic Lift (19 ¾” – 25 ½”) [157MM / G157MM]
* 267 mm Pneumatic Lift (25 ¾” – 35 ¾”) [267MM / G267MM]

Measurements/Overall Dimensions:Boxed Weight/Size: 56 lbs. / 6.7 cu.ft. | Counter Height Mechanism:* Independent Back Angle Adjustment
* Fixed Seat
* Seat Height

**Options:***Midnight Black* * Modified Multi Tilt Mechanism (Seat slider, height and back angle adjustment only) [MT]
* Dedicated Task 2 Mechanism [DT2]

Base/Footring/Glides/Casters:* 26" Glass Reinforced Nylon *(Midnight Black / Light Grey)*
* Aluminum, Height Adjustable Footring (20” Diameter, 1 ¾” Thick Foot Platform)
* 1 ¼” Glides

**Options:*** Lock-On Urethane Casters [LON]
* Lock-Off Urethane Casters [LOF]
* Dual Wheel Nylon Casters [NC]
* Dual Wheel Urethane Casters [UC]
* Single Wheel Nylon Casters [SW]
* Single Wheel Urethane Casters [SWU]
* 2 ¼” Glides [2G]

Additional Options:Midnight Black / Light Grey [G] * Adjustable Headrest [AHR / AHRG]

\*Mixing of Midnight Black & Light Grey components is not an option. |