tCentric Hybrid™

|  |  |
| --- | --- |
| Knee Tilt\* | Midnight Black [t-KT] |
| Backrest:* 5" Patented Back Height Adjustment System
* Dual Curve Mesh Backrest (19"w x 25"h)

Arms: Midnight Black **Options:*** tCentric Armrest Height & Lateral [TCL]
* tCentric Armrest Height & Swivel [TC360]
* tCentric Armrest Height, Lateral & Swivel [TCL360]

Seat:Midnight Black * Dual Density Molded Polyurethane Foam
* Eight ply hardwood seat structure
* Tailored upholstery on seat pan (20”w x 19”d)

**Options:*** Extra Small Seat (17 ½”w x 15 ½”d) [XSS]
* Small Seat (18 ½”w x 17”d) [SS]
* Plus Size Seat (22”w x 19”d) [PS]
* Extra Long Seat (20”w x 21”d) [XLS]
* Extra Deep Seat (22”w x 21”d) [XPS]
* Energy Absorbent Memory Foam [EA]
* Triple Density Foam (adds ¼” to seat width & depth) [TDF]
* Non-tailored Seat Pan [NTS]

Knee Tilt Mechanism:Midnight Black * 5” Incremental Back Height
* Infinite Lock Free Float
* Back Angle
* Spring Tension
* 2 ½” Seat Depth
* Pneumatic Seat Height

Measurements/Overall Dimensions:Boxed Weight/Size: 46.4 lbs. / 11.7 cu.ft. | Pneumatic Lift (Seat Height):Midnight Black * 125 mmLT Pneumatic Lift (18 ¾" – 23 ½")

**Options:***Midnight Black [G]** 70 mm Pneumatic Lift (18 ¼” – 21”) [70MM]
* 80 mm Pneumatic Lift (19”-22”) [80MM]
* 100 mm Pneumatic Lift (19 ½”-23 ¼”) [100MM/G100MM]
* 140 mm Pneumatic Lift (20 ¾”-26 ¼”) [140MM/G140MM]

*Chrome** 100 mm Chrome Pneumatic Lift (19 ½”-23 ¼”) [100MMCH]
* 125 mm Chrome Pneumatic Lift (19 ¾”-24 ½”) [125MMCH]
* 140 mm Chrome Pneumatic Lift (20 ¾”-26 ¼”) [140MMCH]

Base/Glides/Casters:Midnight Black * 26" Glass Reinforced Nylon Mid-Profile Base
* 5 Dual Wheel Nylon Casters 2

**Options:*** Chrome Accent Casters [CAC]
* 26” Polished Aluminum Mid-Profile Base [PMB]
* Dual Wheel Urethane Caster 2 [UC2]

Additional Options: Midnight Black* tCentric Lumbar Support [TLS]
* tCentric Lumbar Support with Air Lumbar (pump) [TLSAL]
* Adjustable Headrest [AHR]
 |

­