tCentric Hybrid™

|  |  |
| --- | --- |
| Synchro Glide | Midnight Black [t-SG] |
| Light Grey [t-SGG] |
| Mixing of Midnight Black & Light Grey components is not an option. |
| Backrest* 5" Patented Back Height Adjustment System
* Dual Curve Mesh Backrest (19"w x 25"h)

Arms (Midnight Black / Light Grey) * [Click here](http://ergocentric.com/resource/arms) to view options

Seat(Midnight Black / Light Grey)* Dual Density Molded Polyurethane Foam
* Eight ply hardwood seat structure
* Tailored upholstery on seat pan (20”w x 19”d)

**Options:*** Extra Small Seat (17.5”w x 15.5”d) [XSS]
* Small Seat (18.5”w x 17”d) [SS]
* Plus Size Seat (22”w x 19”d) [PS]
* Extra Long Seat (20”w x 21”d) [XLS]
* Extra Deep Seat (22”w x 21”d) [XPS]

Pneumatic Lift (Seat Height)(Midnight Black / Light Grey) * 125 mm Pneumatic Lift (18.5" – 23.25")

**Options:***Midnight Black / Light Grey** 80 mm Pneumatic Lift (17.75”-20.75”) [80mm/G80mm]
* 100 mm Pneumatic Lift (18.25”-22”) [100mm/G100mm]
* 140 mm Pneumatic Lift (19.5”-25”) [140mm/G140mm]

*Chrome** 100 mm Chrome Pneumatic Lift (18.25”-22”) [100mmCH]
* 125 mm Chrome Pneumatic Lift (18.5”-23.25”) [125mmCH]
* 140 mm Chrome Pneumatic Lift (19.5”-25”) [140mmCH]
 | Synchro Glide Mechanism(Midnight Black / Light Grey) * 2.5” Depth Adjustable Seat Slider
* Adjustable Spring Tension
* Free Float
* Independent Back Angle Adjustment
* Seat Tilt Lock Out
* Synchro 2:1 Ratio

Base/Glides/Casters*Midnight Black** 26" Glass reinforced nylon high profile base
* 5 Dual wheel nylon casters 2

*Light Grey** 26" Glass reinforced nylon high profile base
* 5 Dual wheel nylon casters 2

**Options:*** Energy Absorbent Memory Foam [EA]
* Triple Density Foam [TDF]
* Non-Tailored Seat Pan [NTS]
* Chrome Accent Casters [CAC]
* 26” Polished Aluminum Base [26PB2]
* Dual Wheel Urethane Caster 2 [UC2]

Additional Options*Midnight Black** Lumbar Support [TLS]
* Air Lumbar [TLSAL]
* Adjustable Headrest [AHRTS]

*Light Grey** Lumbar Support [TLSG]
* Air Lumbar [TLSALG]
* Adjustable Headrest [AHRTSG]
 |